This is Info file gcc.info, produced by Makeinfo version 1.68 from the
input file ../../gcc-2.95.2/gcc/gcc.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gcc: (gcc).                  The GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the use and the internals of the GNU compiler.

   Published by the Free Software Foundation 59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

   Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999 Free Software Foundation, Inc.

   Permission is granted to make and distribute verbatim copies of this
manual provided the copyright notice and this permission notice are
preserved on all copies.

   Permission is granted to copy and distribute modified versions of
this manual under the conditions for verbatim copying, provided also
that the sections entitled "GNU General Public License" and "Funding
for Free Software" are included exactly as in the original, and
provided that the entire resulting derived work is distributed under
the terms of a permission notice identical to this one.

   Permission is granted to copy and distribute translations of this
manual into another language, under the above conditions for modified
versions, except that the sections entitled "GNU General Public
License" and "Funding for Free Software", and this permission notice,
may be included in translations approved by the Free Software Foundation
instead of in the original English.


File: gcc.info,  Node: Trampolines,  Next: Library Calls,  Prev: Varargs,  Up: Target Macros

Trampolines for Nested Functions
================================

   A "trampoline" is a small piece of code that is created at run time
when the address of a nested function is taken.  It normally resides on
the stack, in the stack frame of the containing function.  These macros
tell GNU CC how to generate code to allocate and initialize a
trampoline.

   The instructions in the trampoline must do two things: load a
constant address into the static chain register, and jump to the real
address of the nested function.  On CISC machines such as the m68k,
this requires two instructions, a move immediate and a jump.  Then the
two addresses exist in the trampoline as word-long immediate operands.
On RISC machines, it is often necessary to load each address into a
register in two parts.  Then pieces of each address form separate
immediate operands.

   The code generated to initialize the trampoline must store the
variable parts--the static chain value and the function address--into
the immediate operands of the instructions.  On a CISC machine, this is
simply a matter of copying each address to a memory reference at the
proper offset from the start of the trampoline.  On a RISC machine, it
may be necessary to take out pieces of the address and store them
separately.

`TRAMPOLINE_TEMPLATE (FILE)'
     A C statement to output, on the stream FILE, assembler code for a
     block of data that contains the constant parts of a trampoline.
     This code should not include a label--the label is taken care of
     automatically.

     If you do not define this macro, it means no template is needed
     for the target.  Do not define this macro on systems where the
     block move code to copy the trampoline into place would be larger
     than the code to generate it on the spot.

`TRAMPOLINE_SECTION'
     The name of a subroutine to switch to the section in which the
     trampoline template is to be placed (*note Sections::.).  The
     default is a value of `readonly_data_section', which places the
     trampoline in the section containing read-only data.

`TRAMPOLINE_SIZE'
     A C expression for the size in bytes of the trampoline, as an
     integer.

`TRAMPOLINE_ALIGNMENT'
     Alignment required for trampolines, in bits.

     If you don't define this macro, the value of `BIGGEST_ALIGNMENT'
     is used for aligning trampolines.

`INITIALIZE_TRAMPOLINE (ADDR, FNADDR, STATIC_CHAIN)'
     A C statement to initialize the variable parts of a trampoline.
     ADDR is an RTX for the address of the trampoline; FNADDR is an RTX
     for the address of the nested function; STATIC_CHAIN is an RTX for
     the static chain value that should be passed to the function when
     it is called.

`ALLOCATE_TRAMPOLINE (FP)'
     A C expression to allocate run-time space for a trampoline.  The
     expression value should be an RTX representing a memory reference
     to the space for the trampoline.

     If this macro is not defined, by default the trampoline is
     allocated as a stack slot.  This default is right for most
     machines.  The exceptions are machines where it is impossible to
     execute instructions in the stack area.  On such machines, you may
     have to implement a separate stack, using this macro in
     conjunction with `FUNCTION_PROLOGUE' and `FUNCTION_EPILOGUE'.

     FP points to a data structure, a `struct function', which
     describes the compilation status of the immediate containing
     function of the function which the trampoline is for.  Normally
     (when `ALLOCATE_TRAMPOLINE' is not defined), the stack slot for the
     trampoline is in the stack frame of this containing function.
     Other allocation strategies probably must do something analogous
     with this information.

   Implementing trampolines is difficult on many machines because they
have separate instruction and data caches.  Writing into a stack
location fails to clear the memory in the instruction cache, so when
the program jumps to that location, it executes the old contents.

   Here are two possible solutions.  One is to clear the relevant parts
of the instruction cache whenever a trampoline is set up.  The other is
to make all trampolines identical, by having them jump to a standard
subroutine.  The former technique makes trampoline execution faster; the
latter makes initialization faster.

   To clear the instruction cache when a trampoline is initialized,
define the following macros which describe the shape of the cache.

`INSN_CACHE_SIZE'
     The total size in bytes of the cache.

`INSN_CACHE_LINE_WIDTH'
     The length in bytes of each cache line.  The cache is divided into
     cache lines which are disjoint slots, each holding a contiguous
     chunk of data fetched from memory.  Each time data is brought into
     the cache, an entire line is read at once.  The data loaded into a
     cache line is always aligned on a boundary equal to the line size.

`INSN_CACHE_DEPTH'
     The number of alternative cache lines that can hold any particular
     memory location.

   Alternatively, if the machine has system calls or instructions to
clear the instruction cache directly, you can define the following
macro.

`CLEAR_INSN_CACHE (BEG, END)'
     If defined, expands to a C expression clearing the *instruction
     cache* in the specified interval.  If it is not defined, and the
     macro INSN_CACHE_SIZE is defined, some generic code is generated
     to clear the cache.  The definition of this macro would typically
     be a series of `asm' statements.  Both BEG and END are both pointer
     expressions.

   To use a standard subroutine, define the following macro.  In
addition, you must make sure that the instructions in a trampoline fill
an entire cache line with identical instructions, or else ensure that
the beginning of the trampoline code is always aligned at the same
point in its cache line.  Look in `m68k.h' as a guide.

`TRANSFER_FROM_TRAMPOLINE'
     Define this macro if trampolines need a special subroutine to do
     their work.  The macro should expand to a series of `asm'
     statements which will be compiled with GNU CC.  They go in a
     library function named `__transfer_from_trampoline'.

     If you need to avoid executing the ordinary prologue code of a
     compiled C function when you jump to the subroutine, you can do so
     by placing a special label of your own in the assembler code.  Use
     one `asm' statement to generate an assembler label, and another to
     make the label global.  Then trampolines can use that label to
     jump directly to your special assembler code.


File: gcc.info,  Node: Library Calls,  Next: Addressing Modes,  Prev: Trampolines,  Up: Target Macros

Implicit Calls to Library Routines
==================================

   Here is an explanation of implicit calls to library routines.

`MULSI3_LIBCALL'
     A C string constant giving the name of the function to call for
     multiplication of one signed full-word by another.  If you do not
     define this macro, the default name is used, which is `__mulsi3',
     a function defined in `libgcc.a'.

`DIVSI3_LIBCALL'
     A C string constant giving the name of the function to call for
     division of one signed full-word by another.  If you do not define
     this macro, the default name is used, which is `__divsi3', a
     function defined in `libgcc.a'.

`UDIVSI3_LIBCALL'
     A C string constant giving the name of the function to call for
     division of one unsigned full-word by another.  If you do not
     define this macro, the default name is used, which is `__udivsi3',
     a function defined in `libgcc.a'.

`MODSI3_LIBCALL'
     A C string constant giving the name of the function to call for the
     remainder in division of one signed full-word by another.  If you
     do not define this macro, the default name is used, which is
     `__modsi3', a function defined in `libgcc.a'.

`UMODSI3_LIBCALL'
     A C string constant giving the name of the function to call for the
     remainder in division of one unsigned full-word by another.  If
     you do not define this macro, the default name is used, which is
     `__umodsi3', a function defined in `libgcc.a'.

`MULDI3_LIBCALL'
     A C string constant giving the name of the function to call for
     multiplication of one signed double-word by another.  If you do not
     define this macro, the default name is used, which is `__muldi3',
     a function defined in `libgcc.a'.

`DIVDI3_LIBCALL'
     A C string constant giving the name of the function to call for
     division of one signed double-word by another.  If you do not
     define this macro, the default name is used, which is `__divdi3', a
     function defined in `libgcc.a'.

`UDIVDI3_LIBCALL'
     A C string constant giving the name of the function to call for
     division of one unsigned full-word by another.  If you do not
     define this macro, the default name is used, which is `__udivdi3',
     a function defined in `libgcc.a'.

`MODDI3_LIBCALL'
     A C string constant giving the name of the function to call for the
     remainder in division of one signed double-word by another.  If
     you do not define this macro, the default name is used, which is
     `__moddi3', a function defined in `libgcc.a'.

`UMODDI3_LIBCALL'
     A C string constant giving the name of the function to call for the
     remainder in division of one unsigned full-word by another.  If
     you do not define this macro, the default name is used, which is
     `__umoddi3', a function defined in `libgcc.a'.

`INIT_TARGET_OPTABS'
     Define this macro as a C statement that declares additional library
     routines renames existing ones. `init_optabs' calls this macro
     after initializing all the normal library routines.

`TARGET_EDOM'
     The value of `EDOM' on the target machine, as a C integer constant
     expression.  If you don't define this macro, GNU CC does not
     attempt to deposit the value of `EDOM' into `errno' directly.
     Look in `/usr/include/errno.h' to find the value of `EDOM' on your
     system.

     If you do not define `TARGET_EDOM', then compiled code reports
     domain errors by calling the library function and letting it
     report the error.  If mathematical functions on your system use
     `matherr' when there is an error, then you should leave
     `TARGET_EDOM' undefined so that `matherr' is used normally.

`GEN_ERRNO_RTX'
     Define this macro as a C expression to create an rtl expression
     that refers to the global "variable" `errno'.  (On certain systems,
     `errno' may not actually be a variable.)  If you don't define this
     macro, a reasonable default is used.

`TARGET_MEM_FUNCTIONS'
     Define this macro if GNU CC should generate calls to the System V
     (and ANSI C) library functions `memcpy' and `memset' rather than
     the BSD functions `bcopy' and `bzero'.

`LIBGCC_NEEDS_DOUBLE'
     Define this macro if only `float' arguments cannot be passed to
     library routines (so they must be converted to `double').  This
     macro affects both how library calls are generated and how the
     library routines in `libgcc1.c' accept their arguments.  It is
     useful on machines where floating and fixed point arguments are
     passed differently, such as the i860.

`FLOAT_ARG_TYPE'
     Define this macro to override the type used by the library
     routines to pick up arguments of type `float'.  (By default, they
     use a union of `float' and `int'.)

     The obvious choice would be `float'--but that won't work with
     traditional C compilers that expect all arguments declared as
     `float' to arrive as `double'.  To avoid this conversion, the
     library routines ask for the value as some other type and then
     treat it as a `float'.

     On some systems, no other type will work for this.  For these
     systems, you must use `LIBGCC_NEEDS_DOUBLE' instead, to force
     conversion of the values `double' before they are passed.

`FLOATIFY (PASSED-VALUE)'
     Define this macro to override the way library routines redesignate
     a `float' argument as a `float' instead of the type it was passed
     as.  The default is an expression which takes the `float' field of
     the union.

`FLOAT_VALUE_TYPE'
     Define this macro to override the type used by the library
     routines to return values that ought to have type `float'.  (By
     default, they use `int'.)

     The obvious choice would be `float'--but that won't work with
     traditional C compilers gratuitously convert values declared as
     `float' into `double'.

`INTIFY (FLOAT-VALUE)'
     Define this macro to override the way the value of a
     `float'-returning library routine should be packaged in order to
     return it.  These functions are actually declared to return type
     `FLOAT_VALUE_TYPE' (normally `int').

     These values can't be returned as type `float' because traditional
     C compilers would gratuitously convert the value to a `double'.

     A local variable named `intify' is always available when the macro
     `INTIFY' is used.  It is a union of a `float' field named `f' and
     a field named `i' whose type is `FLOAT_VALUE_TYPE' or `int'.

     If you don't define this macro, the default definition works by
     copying the value through that union.

`nongcc_SI_type'
     Define this macro as the name of the data type corresponding to
     `SImode' in the system's own C compiler.

     You need not define this macro if that type is `long int', as it
     usually is.

`nongcc_word_type'
     Define this macro as the name of the data type corresponding to the
     word_mode in the system's own C compiler.

     You need not define this macro if that type is `long int', as it
     usually is.

`perform_...'
     Define these macros to supply explicit C statements to carry out
     various arithmetic operations on types `float' and `double' in the
     library routines in `libgcc1.c'.  See that file for a full list of
     these macros and their arguments.

     On most machines, you don't need to define any of these macros,
     because the C compiler that comes with the system takes care of
     doing them.

`NEXT_OBJC_RUNTIME'
     Define this macro to generate code for Objective C message sending
     using the calling convention of the NeXT system.  This calling
     convention involves passing the object, the selector and the
     method arguments all at once to the method-lookup library function.

     The default calling convention passes just the object and the
     selector to the lookup function, which returns a pointer to the
     method.


File: gcc.info,  Node: Addressing Modes,  Next: Condition Code,  Prev: Library Calls,  Up: Target Macros

Addressing Modes
================

   This is about addressing modes.

`HAVE_POST_INCREMENT'
     A C expression that is nonzero the machine supports post-increment
     addressing.

`HAVE_PRE_INCREMENT'
`HAVE_POST_DECREMENT'
`HAVE_PRE_DECREMENT'
     Similar for other kinds of addressing.

`CONSTANT_ADDRESS_P (X)'
     A C expression that is 1 if the RTX X is a constant which is a
     valid address.  On most machines, this can be defined as
     `CONSTANT_P (X)', but a few machines are more restrictive in which
     constant addresses are supported.

     `CONSTANT_P' accepts integer-values expressions whose values are
     not explicitly known, such as `symbol_ref', `label_ref', and
     `high' expressions and `const' arithmetic expressions, in addition
     to `const_int' and `const_double' expressions.

`MAX_REGS_PER_ADDRESS'
     A number, the maximum number of registers that can appear in a
     valid memory address.  Note that it is up to you to specify a
     value equal to the maximum number that `GO_IF_LEGITIMATE_ADDRESS'
     would ever accept.

`GO_IF_LEGITIMATE_ADDRESS (MODE, X, LABEL)'
     A C compound statement with a conditional `goto LABEL;' executed
     if X (an RTX) is a legitimate memory address on the target machine
     for a memory operand of mode MODE.

     It usually pays to define several simpler macros to serve as
     subroutines for this one.  Otherwise it may be too complicated to
     understand.

     This macro must exist in two variants: a strict variant and a
     non-strict one.  The strict variant is used in the reload pass.  It
     must be defined so that any pseudo-register that has not been
     allocated a hard register is considered a memory reference.  In
     contexts where some kind of register is required, a pseudo-register
     with no hard register must be rejected.

     The non-strict variant is used in other passes.  It must be
     defined to accept all pseudo-registers in every context where some
     kind of register is required.

     Compiler source files that want to use the strict variant of this
     macro define the macro `REG_OK_STRICT'.  You should use an `#ifdef
     REG_OK_STRICT' conditional to define the strict variant in that
     case and the non-strict variant otherwise.

     Subroutines to check for acceptable registers for various purposes
     (one for base registers, one for index registers, and so on) are
     typically among the subroutines used to define
     `GO_IF_LEGITIMATE_ADDRESS'.  Then only these subroutine macros
     need have two variants; the higher levels of macros may be the
     same whether strict or not.

     Normally, constant addresses which are the sum of a `symbol_ref'
     and an integer are stored inside a `const' RTX to mark them as
     constant.  Therefore, there is no need to recognize such sums
     specifically as legitimate addresses.  Normally you would simply
     recognize any `const' as legitimate.

     Usually `PRINT_OPERAND_ADDRESS' is not prepared to handle constant
     sums that are not marked with  `const'.  It assumes that a naked
     `plus' indicates indexing.  If so, then you *must* reject such
     naked constant sums as illegitimate addresses, so that none of
     them will be given to `PRINT_OPERAND_ADDRESS'.

     On some machines, whether a symbolic address is legitimate depends
     on the section that the address refers to.  On these machines,
     define the macro `ENCODE_SECTION_INFO' to store the information
     into the `symbol_ref', and then check for it here.  When you see a
     `const', you will have to look inside it to find the `symbol_ref'
     in order to determine the section.  *Note Assembler Format::.

     The best way to modify the name string is by adding text to the
     beginning, with suitable punctuation to prevent any ambiguity.
     Allocate the new name in `saveable_obstack'.  You will have to
     modify `ASM_OUTPUT_LABELREF' to remove and decode the added text
     and output the name accordingly, and define `STRIP_NAME_ENCODING'
     to access the original name string.

     You can check the information stored here into the `symbol_ref' in
     the definitions of the macros `GO_IF_LEGITIMATE_ADDRESS' and
     `PRINT_OPERAND_ADDRESS'.

`REG_OK_FOR_BASE_P (X)'
     A C expression that is nonzero if X (assumed to be a `reg' RTX) is
     valid for use as a base register.  For hard registers, it should
     always accept those which the hardware permits and reject the
     others.  Whether the macro accepts or rejects pseudo registers
     must be controlled by `REG_OK_STRICT' as described above.  This
     usually requires two variant definitions, of which `REG_OK_STRICT'
     controls the one actually used.

`REG_MODE_OK_FOR_BASE_P (X, MODE)'
     A C expression that is just like `REG_OK_FOR_BASE_P', except that
     that expression may examine the mode of the memory reference in
     MODE.  You should define this macro if the mode of the memory
     reference affects whether a register may be used as a base
     register.  If you define this macro, the compiler will use it
     instead of `REG_OK_FOR_BASE_P'.

`REG_OK_FOR_INDEX_P (X)'
     A C expression that is nonzero if X (assumed to be a `reg' RTX) is
     valid for use as an index register.

     The difference between an index register and a base register is
     that the index register may be scaled.  If an address involves the
     sum of two registers, neither one of them scaled, then either one
     may be labeled the "base" and the other the "index"; but whichever
     labeling is used must fit the machine's constraints of which
     registers may serve in each capacity.  The compiler will try both
     labelings, looking for one that is valid, and will reload one or
     both registers only if neither labeling works.

`LEGITIMIZE_ADDRESS (X, OLDX, MODE, WIN)'
     A C compound statement that attempts to replace X with a valid
     memory address for an operand of mode MODE.  WIN will be a C
     statement label elsewhere in the code; the macro definition may use

          GO_IF_LEGITIMATE_ADDRESS (MODE, X, WIN);

     to avoid further processing if the address has become legitimate.

     X will always be the result of a call to `break_out_memory_refs',
     and OLDX will be the operand that was given to that function to
     produce X.

     The code generated by this macro should not alter the substructure
     of X.  If it transforms X into a more legitimate form, it should
     assign X (which will always be a C variable) a new value.

     It is not necessary for this macro to come up with a legitimate
     address.  The compiler has standard ways of doing so in all cases.
     In fact, it is safe for this macro to do nothing.  But often a
     machine-dependent strategy can generate better code.

`LEGITIMIZE_RELOAD_ADDRESS (X, MODE, OPNUM, TYPE, IND_LEVELS, WIN)'
     A C compound statement that attempts to replace X, which is an
     address that needs reloading, with a valid memory address for an
     operand of mode MODE.  WIN will be a C statement label elsewhere
     in the code.  It is not necessary to define this macro, but it
     might be useful for performance reasons.

     For example, on the i386, it is sometimes possible to use a single
     reload register instead of two by reloading a sum of two pseudo
     registers into a register.  On the other hand, for number of RISC
     processors offsets are limited so that often an intermediate
     address needs to be generated in order to address a stack slot.
     By defining LEGITIMIZE_RELOAD_ADDRESS appropriately, the
     intermediate addresses generated for adjacent some stack slots can
     be made identical, and thus be shared.

     *Note*: This macro should be used with caution.  It is necessary
     to know something of how reload works in order to effectively use
     this, and it is quite easy to produce macros that build in too
     much knowledge of reload internals.

     *Note*: This macro must be able to reload an address created by a
     previous invocation of this macro.  If it fails to handle such
     addresses then the compiler may generate incorrect code or abort.

     The macro definition should use `push_reload' to indicate parts
     that need reloading; OPNUM, TYPE and IND_LEVELS are usually
     suitable to be passed unaltered to `push_reload'.

     The code generated by this macro must not alter the substructure of
     X.  If it transforms X into a more legitimate form, it should
     assign X (which will always be a C variable) a new value.  This
     also applies to parts that you change indirectly by calling
     `push_reload'.

     The macro definition may use `strict_memory_address_p' to test if
     the address has become legitimate.

     If you want to change only a part of X, one standard way of doing
     this is to use `copy_rtx'.  Note, however, that is unshares only a
     single level of rtl.  Thus, if the part to be changed is not at the
     top level, you'll need to replace first the top leve It is not
     necessary for this macro to come up with a legitimate address;
     but often a machine-dependent strategy can generate better code.

`GO_IF_MODE_DEPENDENT_ADDRESS (ADDR, LABEL)'
     A C statement or compound statement with a conditional `goto
     LABEL;' executed if memory address X (an RTX) can have different
     meanings depending on the machine mode of the memory reference it
     is used for or if the address is valid for some modes but not
     others.

     Autoincrement and autodecrement addresses typically have
     mode-dependent effects because the amount of the increment or
     decrement is the size of the operand being addressed.  Some
     machines have other mode-dependent addresses.  Many RISC machines
     have no mode-dependent addresses.

     You may assume that ADDR is a valid address for the machine.

`LEGITIMATE_CONSTANT_P (X)'
     A C expression that is nonzero if X is a legitimate constant for
     an immediate operand on the target machine.  You can assume that X
     satisfies `CONSTANT_P', so you need not check this.  In fact, `1'
     is a suitable definition for this macro on machines where anything
     `CONSTANT_P' is valid.


File: gcc.info,  Node: Condition Code,  Next: Costs,  Prev: Addressing Modes,  Up: Target Macros

Condition Code Status
=====================

   This describes the condition code status.

   The file `conditions.h' defines a variable `cc_status' to describe
how the condition code was computed (in case the interpretation of the
condition code depends on the instruction that it was set by).  This
variable contains the RTL expressions on which the condition code is
currently based, and several standard flags.

   Sometimes additional machine-specific flags must be defined in the
machine description header file.  It can also add additional
machine-specific information by defining `CC_STATUS_MDEP'.

`CC_STATUS_MDEP'
     C code for a data type which is used for declaring the `mdep'
     component of `cc_status'.  It defaults to `int'.

     This macro is not used on machines that do not use `cc0'.

`CC_STATUS_MDEP_INIT'
     A C expression to initialize the `mdep' field to "empty".  The
     default definition does nothing, since most machines don't use the
     field anyway.  If you want to use the field, you should probably
     define this macro to initialize it.

     This macro is not used on machines that do not use `cc0'.

`NOTICE_UPDATE_CC (EXP, INSN)'
     A C compound statement to set the components of `cc_status'
     appropriately for an insn INSN whose body is EXP.  It is this
     macro's responsibility to recognize insns that set the condition
     code as a byproduct of other activity as well as those that
     explicitly set `(cc0)'.

     This macro is not used on machines that do not use `cc0'.

     If there are insns that do not set the condition code but do alter
     other machine registers, this macro must check to see whether they
     invalidate the expressions that the condition code is recorded as
     reflecting.  For example, on the 68000, insns that store in address
     registers do not set the condition code, which means that usually
     `NOTICE_UPDATE_CC' can leave `cc_status' unaltered for such insns.
     But suppose that the previous insn set the condition code based
     on location `a4@(102)' and the current insn stores a new value in
     `a4'.  Although the condition code is not changed by this, it will
     no longer be true that it reflects the contents of `a4@(102)'.
     Therefore, `NOTICE_UPDATE_CC' must alter `cc_status' in this case
     to say that nothing is known about the condition code value.

     The definition of `NOTICE_UPDATE_CC' must be prepared to deal with
     the results of peephole optimization: insns whose patterns are
     `parallel' RTXs containing various `reg', `mem' or constants which
     are just the operands.  The RTL structure of these insns is not
     sufficient to indicate what the insns actually do.  What
     `NOTICE_UPDATE_CC' should do when it sees one is just to run
     `CC_STATUS_INIT'.

     A possible definition of `NOTICE_UPDATE_CC' is to call a function
     that looks at an attribute (*note Insn Attributes::.) named, for
     example, `cc'.  This avoids having detailed information about
     patterns in two places, the `md' file and in `NOTICE_UPDATE_CC'.

`EXTRA_CC_MODES'
     A list of names to be used for additional modes for condition code
     values in registers (*note Jump Patterns::.).  These names are
     added to `enum machine_mode' and all have class `MODE_CC'.  By
     convention, they should start with `CC' and end with `mode'.

     You should only define this macro if your machine does not use
     `cc0' and only if additional modes are required.

`EXTRA_CC_NAMES'
     A list of C strings giving the names for the modes listed in
     `EXTRA_CC_MODES'.  For example, the Sparc defines this macro and
     `EXTRA_CC_MODES' as

          #define EXTRA_CC_MODES CC_NOOVmode, CCFPmode, CCFPEmode
          #define EXTRA_CC_NAMES "CC_NOOV", "CCFP", "CCFPE"

     This macro is not required if `EXTRA_CC_MODES' is not defined.

`SELECT_CC_MODE (OP, X, Y)'
     Returns a mode from class `MODE_CC' to be used when comparison
     operation code OP is applied to rtx X and Y.  For example, on the
     Sparc, `SELECT_CC_MODE' is defined as (see *note Jump Patterns::.
     for a description of the reason for this definition)

          #define SELECT_CC_MODE(OP,X,Y) \
            (GET_MODE_CLASS (GET_MODE (X)) == MODE_FLOAT          \
             ? ((OP == EQ || OP == NE) ? CCFPmode : CCFPEmode)    \
             : ((GET_CODE (X) == PLUS || GET_CODE (X) == MINUS    \
                 || GET_CODE (X) == NEG) \
                ? CC_NOOVmode : CCmode))

     You need not define this macro if `EXTRA_CC_MODES' is not defined.

`CANONICALIZE_COMPARISON (CODE, OP0, OP1)'
     One some machines not all possible comparisons are defined, but
     you can convert an invalid comparison into a valid one.  For
     example, the Alpha does not have a `GT' comparison, but you can
     use an `LT' comparison instead and swap the order of the operands.

     On such machines, define this macro to be a C statement to do any
     required conversions.  CODE is the initial comparison code and OP0
     and OP1 are the left and right operands of the comparison,
     respectively.  You should modify CODE, OP0, and OP1 as required.

     GNU CC will not assume that the comparison resulting from this
     macro is valid but will see if the resulting insn matches a
     pattern in the `md' file.

     You need not define this macro if it would never change the
     comparison code or operands.

`REVERSIBLE_CC_MODE (MODE)'
     A C expression whose value is one if it is always safe to reverse a
     comparison whose mode is MODE.  If `SELECT_CC_MODE' can ever
     return MODE for a floating-point inequality comparison, then
     `REVERSIBLE_CC_MODE (MODE)' must be zero.

     You need not define this macro if it would always returns zero or
     if the floating-point format is anything other than
     `IEEE_FLOAT_FORMAT'.  For example, here is the definition used on
     the Sparc, where floating-point inequality comparisons are always
     given `CCFPEmode':

          #define REVERSIBLE_CC_MODE(MODE)  ((MODE) != CCFPEmode)


File: gcc.info,  Node: Costs,  Next: Sections,  Prev: Condition Code,  Up: Target Macros

Describing Relative Costs of Operations
=======================================

   These macros let you describe the relative speed of various
operations on the target machine.

`CONST_COSTS (X, CODE, OUTER_CODE)'
     A part of a C `switch' statement that describes the relative costs
     of constant RTL expressions.  It must contain `case' labels for
     expression codes `const_int', `const', `symbol_ref', `label_ref'
     and `const_double'.  Each case must ultimately reach a `return'
     statement to return the relative cost of the use of that kind of
     constant value in an expression.  The cost may depend on the
     precise value of the constant, which is available for examination
     in X, and the rtx code of the expression in which it is contained,
     found in OUTER_CODE.

     CODE is the expression code--redundant, since it can be obtained
     with `GET_CODE (X)'.

`RTX_COSTS (X, CODE, OUTER_CODE)'
     Like `CONST_COSTS' but applies to nonconstant RTL expressions.
     This can be used, for example, to indicate how costly a multiply
     instruction is.  In writing this macro, you can use the construct
     `COSTS_N_INSNS (N)' to specify a cost equal to N fast
     instructions.  OUTER_CODE is the code of the expression in which X
     is contained.

     This macro is optional; do not define it if the default cost
     assumptions are adequate for the target machine.

`DEFAULT_RTX_COSTS (X, CODE, OUTER_CODE)'
     This macro, if defined, is called for any case not handled by the
     `RTX_COSTS' or `CONST_COSTS' macros.  This eliminates the need to
     put case labels into the macro, but the code, or any functions it
     calls, must assume that the RTL in X could be of any type that has
     not already been handled.  The arguments are the same as for
     `RTX_COSTS', and the macro should execute a return statement giving
     the cost of any RTL expressions that it can handle.  The default
     cost calculation is used for any RTL for which this macro does not
     return a value.

     This macro is optional; do not define it if the default cost
     assumptions are adequate for the target machine.

`ADDRESS_COST (ADDRESS)'
     An expression giving the cost of an addressing mode that contains
     ADDRESS.  If not defined, the cost is computed from the ADDRESS
     expression and the `CONST_COSTS' values.

     For most CISC machines, the default cost is a good approximation
     of the true cost of the addressing mode.  However, on RISC
     machines, all instructions normally have the same length and
     execution time.  Hence all addresses will have equal costs.

     In cases where more than one form of an address is known, the form
     with the lowest cost will be used.  If multiple forms have the
     same, lowest, cost, the one that is the most complex will be used.

     For example, suppose an address that is equal to the sum of a
     register and a constant is used twice in the same basic block.
     When this macro is not defined, the address will be computed in a
     register and memory references will be indirect through that
     register.  On machines where the cost of the addressing mode
     containing the sum is no higher than that of a simple indirect
     reference, this will produce an additional instruction and
     possibly require an additional register.  Proper specification of
     this macro eliminates this overhead for such machines.

     Similar use of this macro is made in strength reduction of loops.

     ADDRESS need not be valid as an address.  In such a case, the cost
     is not relevant and can be any value; invalid addresses need not be
     assigned a different cost.

     On machines where an address involving more than one register is as
     cheap as an address computation involving only one register,
     defining `ADDRESS_COST' to reflect this can cause two registers to
     be live over a region of code where only one would have been if
     `ADDRESS_COST' were not defined in that manner.  This effect should
     be considered in the definition of this macro.  Equivalent costs
     should probably only be given to addresses with different numbers
     of registers on machines with lots of registers.

     This macro will normally either not be defined or be defined as a
     constant.

`REGISTER_MOVE_COST (FROM, TO)'
     A C expression for the cost of moving data from a register in class
     FROM to one in class TO.  The classes are expressed using the
     enumeration values such as `GENERAL_REGS'.  A value of 2 is the
     default; other values are interpreted relative to that.

     It is not required that the cost always equal 2 when FROM is the
     same as TO; on some machines it is expensive to move between
     registers if they are not general registers.

     If reload sees an insn consisting of a single `set' between two
     hard registers, and if `REGISTER_MOVE_COST' applied to their
     classes returns a value of 2, reload does not check to ensure that
     the constraints of the insn are met.  Setting a cost of other than
     2 will allow reload to verify that the constraints are met.  You
     should do this if the `movM' pattern's constraints do not allow
     such copying.

`MEMORY_MOVE_COST (MODE, CLASS, IN)'
     A C expression for the cost of moving data of mode MODE between a
     register of class CLASS and memory; IN is zero if the value is to
     be written to memory, non-zero if it is to be read in.  This cost
     is relative to those in `REGISTER_MOVE_COST'.  If moving between
     registers and memory is more expensive than between two registers,
     you should define this macro to express the relative cost.

     If you do not define this macro, GNU CC uses a default cost of 4
     plus the cost of copying via a secondary reload register, if one is
     needed.  If your machine requires a secondary reload register to
     copy between memory and a register of CLASS but the reload
     mechanism is more complex than copying via an intermediate, define
     this macro to reflect the actual cost of the move.

     GNU CC defines the function `memory_move_secondary_cost' if
     secondary reloads are needed.  It computes the costs due to
     copying via a secondary register.  If your machine copies from
     memory using a secondary register in the conventional way but the
     default base value of 4 is not correct for your machine, define
     this macro to add some other value to the result of that function.
     The arguments to that function are the same as to this macro.

`BRANCH_COST'
     A C expression for the cost of a branch instruction.  A value of 1
     is the default; other values are interpreted relative to that.

   Here are additional macros which do not specify precise relative
costs, but only that certain actions are more expensive than GNU CC
would ordinarily expect.

`SLOW_BYTE_ACCESS'
     Define this macro as a C expression which is nonzero if accessing
     less than a word of memory (i.e. a `char' or a `short') is no
     faster than accessing a word of memory, i.e., if such access
     require more than one instruction or if there is no difference in
     cost between byte and (aligned) word loads.

     When this macro is not defined, the compiler will access a field by
     finding the smallest containing object; when it is defined, a
     fullword load will be used if alignment permits.  Unless bytes
     accesses are faster than word accesses, using word accesses is
     preferable since it may eliminate subsequent memory access if
     subsequent accesses occur to other fields in the same word of the
     structure, but to different bytes.

`SLOW_ZERO_EXTEND'
     Define this macro if zero-extension (of a `char' or `short' to an
     `int') can be done faster if the destination is a register that is
     known to be zero.

     If you define this macro, you must have instruction patterns that
     recognize RTL structures like this:

          (set (strict_low_part (subreg:QI (reg:SI ...) 0)) ...)

     and likewise for `HImode'.

`SLOW_UNALIGNED_ACCESS'
     Define this macro to be the value 1 if unaligned accesses have a
     cost many times greater than aligned accesses, for example if they
     are emulated in a trap handler.

     When this macro is non-zero, the compiler will act as if
     `STRICT_ALIGNMENT' were non-zero when generating code for block
     moves.  This can cause significantly more instructions to be
     produced.  Therefore, do not set this macro non-zero if unaligned
     accesses only add a cycle or two to the time for a memory access.

     If the value of this macro is always zero, it need not be defined.

`DONT_REDUCE_ADDR'
     Define this macro to inhibit strength reduction of memory
     addresses.  (On some machines, such strength reduction seems to do
     harm rather than good.)

`MOVE_RATIO'
     The threshold of number of scalar memory-to-memory move insns,
     *below* which a sequence of insns  should be generated instead of a
     string move insn or a library call.  Increasing the value will
     always make code faster, but eventually incurs high cost in
     increased code size.

     Note that on machines with no memory-to-memory move insns, this
     macro denotes the corresponding number of memory-to-memory
     *sequences*.

     If you don't define this, a reasonable default is used.

`MOVE_BY_PIECES_P (SIZE, ALIGNMENT)'
     A C expression used to determine whether `move_by_pieces' will be
     used to copy a chunk of memory, or whether some other block move
     mechanism will be used.  Defaults to 1 if `move_by_pieces_ninsns'
     returns less than `MOVE_RATIO'.

`MOVE_MAX_PIECES'
     A C expression used by `move_by_pieces' to determine the largest
     unit a load or store used to copy memory is.  Defaults to
     `MOVE_MAX'.

`USE_LOAD_POST_INCREMENT (MODE)'
     A C expression used to determine whether a load postincrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_POST_INCREMENT'.

`USE_LOAD_POST_DECREMENT (MODE)'
     A C expression used to determine whether a load postdecrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_POST_DECREMENT'.

`USE_LOAD_PRE_INCREMENT (MODE)'
     A C expression used to determine whether a load preincrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_PRE_INCREMENT'.

`USE_LOAD_PRE_DECREMENT (MODE)'
     A C expression used to determine whether a load predecrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_PRE_DECREMENT'.

`USE_STORE_POST_INCREMENT (MODE)'
     A C expression used to determine whether a store postincrement is
     a good thing to use for a given mode.  Defaults to the value of
     `HAVE_POST_INCREMENT'.

`USE_STORE_POST_DECREMENT (MODE)'
     A C expression used to determine whether a store postdeccrement is
     a good thing to use for a given mode.  Defaults to the value of
     `HAVE_POST_DECREMENT'.

`USE_STORE_PRE_INCREMENT (MODE)'
     This macro is used to determine whether a store preincrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_PRE_INCREMENT'.

`USE_STORE_PRE_DECREMENT (MODE)'
     This macro is used to determine whether a store predecrement is a
     good thing to use for a given mode.  Defaults to the value of
     `HAVE_PRE_DECREMENT'.

`NO_FUNCTION_CSE'
     Define this macro if it is as good or better to call a constant
     function address than to call an address kept in a register.

`NO_RECURSIVE_FUNCTION_CSE'
     Define this macro if it is as good or better for a function to call
     itself with an explicit address than to call an address kept in a
     register.

`ADJUST_COST (INSN, LINK, DEP_INSN, COST)'
     A C statement (sans semicolon) to update the integer variable COST
     based on the relationship between INSN that is dependent on
     DEP_INSN through the dependence LINK.  The default is to make no
     adjustment to COST.  This can be used for example to specify to
     the scheduler that an output- or anti-dependence does not incur
     the same cost as a data-dependence.

`ADJUST_PRIORITY (INSN)'
     A C statement (sans semicolon) to update the integer scheduling
     priority `INSN_PRIORITY(INSN)'.  Reduce the priority to execute
     the INSN earlier, increase the priority to execute INSN later.
     Do not define this macro if you do not need to adjust the
     scheduling priorities of insns.

